[config_defaults]
path_default_noise 	= detectors\RF\noise
path_default_beep 	= detectors\RF\beep_02
path_sound_on 		= detectors\RF\on
path_sound_off 		= detectors\RF\off
rf_scan_time 		= 5000 ; time in ms between RF signal scans
rf_min_gap 			= 400 ; minimum time in ms between beeps so the sound doesn't get spammed
rf_min_flash_time 	= 100
rf_freq_max 		= 999 ; just a default, MCM will override this if installed
tb_beep				= detectors\tb_detector_radio_beep
indicator_file 		= rax_rf_indicator.xml